**Highlights**

* NDVI from infrared converted camera consistently lower than reference measurements.
* Vegetation shows overestimated reflectance in the converted camera’s red channel.
* Lower cost RGB converted cameras might have systematic measurement errors.
* Studies using drone-camera systems need to consider possible sensor biases.